
全站仪传输软件使用说明

1、从全站仪导出数据
   1）选择正确的串口号，并在仪器和传输软件上选择一致的波特率；
   2）点击传输软件上的【接收】，然后在仪器上点击【发送】或者【导出】；
   3）传输结束后传输软件根据接收的数据类型自动选择对应的显示方式。

2、发送数据到全站仪
   1）选择正确的串口号，并在仪器和传输软件上选择一致的波特率；
   2）打开或直接编辑好需要发送的坐标(仅数值)或者编码（仅字母和数字）文件；
   3）在仪器上进入导入界面，并选择正确的导入数据类型；
   4）在仪器上点击【导入】，然后在传输软件上点击【发送】。

3、设置
   点击【设置】进入设置界面：
   1）角度单位：有度分秒、GON、MIL三种模式，影响测量文件的显示；
   2）距离单位：有米、美国英尺、国际英尺三种模式，影响测量文件和坐标点文件的显示；
   3）坐标顺序：分为NEZ和ENZ两种，改变坐标点显示界面的坐标顺序；
   4）两差系数：0.00、0.14、0.20，影响GTS-7测量数据中平距的计算；
   5）格网因子：范围从0.9-0.11，影响GTS-7测量数据中平距的计算。

4、打开文件
   1）点击【打开】，选择目标文件，软件将根据文件内容自动选择显示模式，其中测量文件以文本形式显示，坐标文件和代码文件以表格形式显示；
   2）支持打开的文件类型有：
          工作文件（*.htf）、
          二进制测量文件（*.mea、*.job、*.dat）、
          二进制坐标文件（*.coo、*.pts、*.cor）、        
          CASS格式已知点文件（*.dat、*.csv、*.txt）、
          GTS-7格式已知点文件（*.csv、*.txt）、
          编码文件（*.txt）；
   3）当打开不支持的文件格式或者文件损坏时显示错误。

5、保存数据
   1）点击保存，当显示区存在数据则根据当前显示的数据内容存储； 
   2）显示的数据类型和保存选项
      测量数据：
          逗号分隔符测量文件（*.csv、*.txt）、
          CASS格式已知点文件（*.dat）、
          DXF已知点文件（*.dxf）、
          GTS-7边角测量数据文件·平距（*.gt7）、
          GTS-7边角测量数据文件·斜距（*.gt7）、
          GTS-7所有测量数据文件（*.gt7）、
          GTS-7格式已知点文件（*.txt）、          
          工作文件（*.htf）；
      坐标数据：
          CASS格式已知点文件（*.dat、*.csv、*.txt）、
          DXF已知点文件（*.dxf）、
          GTS-7格式已知点文件（*.txt）；
      编码文件：
          编码文件（*.txt）；

6、其他
CASS格式坐标点字段    ：点号，编码，X(E),Y(N),Z
GTS-7格式坐标点字段   ：点号，X(E),Y(N),Z，编码
逗号分隔符测量文件字段：STA,点号,仪器高,编码,X(E),Y(N),Z
                        SC,点号,目标好,编码,平距,高差,斜距,X(E),Y(N),Z
   
==================================
PC Port II Instructions

1. Receive data from the total station
   1) Choose the right ComPort. Then choose the same BaudRate on the total station and PC Port II.
   2) Click "Receive" on the PC Port II and then Click "Send" or "Export" on the total station.
   3) The PC Port II will automatically choose the corresponding display mode to show the received data depending on the it's type.

2. Send data to the total station
   1) Choose the right ComPort. Then choose the same BaudRate on the total station and PC Port II.
   2) Edit coordinates file or codes files.
   3) Click "Send" on the PC Port II and then Click "Receive" or "Import" on the total station.

3. Setting
   Click "Setting" to enter setup interface.
   1) Angle Unit: Include DMS, GON and MIL. The angle unit will affect the display of the measured file.   2) Dist Unit:  Include Meter, US-Ft and INT-Ft.The distance unit will affect the display of the measured file and coordinate file.
   3) K Option: Include 0.00, 0.14 and 0.20. The K Option will affect the calculation of horizontal distance in the GTS-7 measured data.
   4) Grid Scale: Range 0.9 to 1.1. The Grid Scale will affect the calculation of horizontal distance in the GTS-7 measured data.
   5) Coord Order: Include NEZ and ENZ.This setting will change the coordinate's order of the coordinate display mode.

4. Open the file
   1) Click "open". Select the target file. The PC Port II will open the file and then automatically display the data according to the file content. The measured data display in the Memo, and the coordinate data and code data display in the Table.
   2) Open options.:
        Any File(*.*),
        CASS coordinate file(*.dat;*.csv;*.txt),
        Binary coordinate file(*.coo;*.pts;*.cor),
        Binary measured File(*.mea;*.job),
        GTS-7 coordinate file(*.csv;*.txt)|,
        TS job file(*.htf),
        Code file(*.txt).
   3) When the format of the file is unsupported or the file is damaged,  show the error message.

5. Save the data
   1) Click "save". If there is data in the display area, The PC Port II will choose the right save options to save the data according to the current data content.
   2) Data types and save options.
      Measured data:
        Comma separator measured file(*.csv),
        Comma separator measured file(*.txt),
        CASS coordinate file(*.dat),
        DXF coordinate file(*.dxf),
        GTS-7 measured file with HD(*.gt7),
        GTS-7 measured file with SD(*.gt7),
        GTS-7 measured file with all data(*.gt7),
        GTS-7 coordinate File(*.txt),
        TS job file(*. htf).
      Coordinate data: 
        CASS coordinate file(*.dat),
        DXF coordinate file(*.dxf),
        CASS coordinate file(*.txt),
        CASS coordinate file(*.csv),
        GTS-7 coordinate File(*.txt);
      Code data:
        Code file(*.txt),
        Any file(*.*).
6. The others
CASS coordinate file：pt no,pt code,X(E),Y(N),Z
GTS-7 coordinate File：pt no,X(E),Y(N),Z,pt code
Comma separator measured file：
STA,pt no,IH,pt code,X(E),Y(N),Z
SC,pt no,TH,pt code,HA,VA,SD,X(E),Y(N),Z
 






