Menu item | Command | Description

Calculate bricks | koplaag | Calculate kop and lagenmaten. First choose the defining dimension with the command KT (kop totaal). This initializes further settings for the other commands. (This command is in Dutch.)
Draw bricklayers on polyline | db | Draw bricklayers only on polylines, which can consists of lines and arcs. For polylines, which only contains horizontal lines, you can also specify a height of the brick wall which will be drawn above. If comment actions is checked, all the calculated measurements are displayed in the text screen. Other options include tile pattern and to start with a whole block